# **SMARTFARMER – IOT ENABLED SMART FARMING APPLICATION**

**Team ID : PNT2022TMID27179**

1. **LED**

import RPi.GPIO as GPIO

from *time* import sleep

GPIO.setwarnings(False)

GPIO.setmode(GPIO.BOARD)

GPIO.setup(8, GPIO.OUT, initial=GPIO.LOW)

value to low (off)

while True:

GPIO.output(8, GPIO.HIGH)

sleep(1)

GPIO.output(8, GPIO.LOW)

sleep(1)

1. **Traffic Light**

from gpiozero import Button, TrafficLights, Buzzer

from time import sleep

buzzer = Buzzer(15)

button = Button(21)

lights = TrafficLights(25, 8, 7)

while True:

button.wait\_for\_press()

buzzer.on()

light.green.on()

sleep(1)

lights.amber.on()

sleep(1)

lights.red.on()

sleep(1)

lights.off()

buzzer.off()